Void spi\_init (void)

{

1-choose spi master or spi slave system

2-configuration spi (clock , clock polarity, clock phase )

3-configuration pins (input and output) (ss,mosi,miso,clk)

4-enable spi

{